**Theatre/Staging Rigging Annual Inspection Checklist**

**HEMP RIGGING SYSTEM**

***Instructions:* 1) Inspect each component listed in the “description” column for damage/function. 2) Place a “checkmark” if the component passes. 3) Place an “X” if the component fails. 3a) If component fails complete the “notes” section below. 4) Write “N/A” if component is not part of the rigging system.**

|  |  |  |
| --- | --- | --- |
| ***Facility Name:*** | ***Inspected by:*** | ***Date:*** |
| **Description** | **Lineset #** | **Lineset #** | **Lineset #** | **Lineset #** | **Lineset #** | **Lineset #** | **Lineset #** | **Lineset #** | **Lineset #** | **Lineset #** |
| Head Block |  |  |  |  |  |  |  |  |  |  |
| Loft Block |  |  |  |  |  |  |  |  |  |  |
| Pin Rail |  |  |  |  |  |  |  |  |  |  |
| Belaying Pins |  |  |  |  |  |  |  |  |  |  |
| Sandbags |  |  |  |  |  |  |  |  |  |  |
| Trim Clamps |  |  |  |  |  |  |  |  |  |  |
| Rope condition |  |  |  |  |  |  |  |  |  |  |
| Batten |  |  |  |  |  |  |  |  |  |  |
| Connection at Batten/Termination |  |  |  |  |  |  |  |  |  |  |
| **Note:**1. **Deficiency -**
2. **Corrective Action -**
3. **Date Corrective Action completed -**
 |